

$Crude Fiber \left(\%\right)=\frac{Loss in weight on ignition}{Weight of the sample}$×100