|  |
| --- |
| **Supplement 1. Three detailed criteria for the Korean minimum housing standard** |
| Minimum residential area and number of rooms | Minimum residential area |  1~6 people | 55㎡ |
|  7~9 people | 64㎡ |
| Number of rooms |  1~2 people | 1 room |
| 3 people | 2 rooms |
| 4~5 people | 3 rooms |
| 6~8 people | 4 rooms |
| 9 people | 5 rooms |
| Essential facility standards |  Single water and sewage, single standing kitchen, single flush toilet, single bath facilities  |
| Environmental standards | Heat resistance; fire resistance; heat dissipation; moisture-proofing;soundproofing; ventilation; lighting; heating facilities;noise; vibration; odor; air pollution;natural disasters such as tidal waves, floods, mountain accidents, cliff collapse |
|