|  |  |  |  |
| --- | --- | --- | --- |
| **Supplement 1. Three detailed criteria for the Korean minimum housing standard** | | | |
| Minimum residential area and  number of rooms | Minimum  residential area | 1~6 people | 55㎡ |
| 7~9 people | 64㎡ |
| Number  of rooms | 1~2 people | 1 room |
| 3 people | 2 rooms |
| 4~5 people | 3 rooms |
| 6~8 people | 4 rooms |
| 9 people | 5 rooms |
| Essential facility standards | | Single water and sewage, single standing kitchen, single flush toilet, single bath facilities | |
| Environmental standards | | Heat resistance; fire resistance; heat dissipation; moisture-proofing; soundproofing; ventilation; lighting; heating facilities; noise; vibration; odor; air pollution; natural disasters such as tidal waves, floods, mountain accidents, cliff collapse | |
|